`

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change Status** | | | | | | | |
| Issue Date | Version | | Summary | | | | Remark |
| 2020-03-18 | A0 | | Document Issue | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
|  |  | |  | | | |  |
| Approved By | | | Checked By | | Prepared By | | |
|  | | |  | |  | | |
| Copy File Department Distribution Detail | | | | | | | |
| Quality Dept. | |  | | SD | |  | |
| Pur. Dept. | |  | |  | |  | |
| Engineering Dept. | |  | |  | |  | |
| MD | |  | |  | |  | |
| This document is stamped with the issuing and issuing date. | | | | | | | |

1. Purchase: In order to declare the TPD demand
2. Function: The document is prepared by the market department.


3、Detail Content :

a). Install coil: Take out the coil ,and Insert the coil from the bottom of the pod

b). Fill e-liquid: Pull out the silica gel plug according to the instructions, then refill e-liquid from oil-filling slots. It is recommended to keep two thirds full.

c). Install the atomizer: Insert the atomizer with e-liquid into the mod.

d). Start to use the device: After keeping it stand for about five minutes, you are free to use the device. You can rotate the pod 180°to adjust the airflow in order to enjoy potimal vaping experience.



e) Application of Product: GEEKVAPE H45 Classic